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[bookmark: _Toc80726007][bookmark: _Toc108882361]Revision Date ___________________________
Berg Mountain Homes feels that it is very important to listen carefully to a customer’s
wishes. At our initial meeting, we discussed many of your goals and wishes for your
future home. The goal of this proposal is to translate those wishes into a working
document that will accurately translate those wishes into working specifications.
This proposal is meant to be a working document. Note that at the end of each section,
there may be a series of comments or questions for you in red. Please respond or add
your own questions and comments in blue.
Your project won’t go to pricing until the specifications are pretty much finalized.
Specifications that will be determined later will be noted as such, but these are usually
items that won’t affect pricing.
Accuracy and detail in this proposal is important for several reasons:
1. Uncertainty causes pricing risk for the builder and that risk is mitigated with
cushion or padding in the price. Accuracy and detail eliminate this risk and
effectively lowers the price of the home.
2. There are a vast number of details that eventually have to be gathered in order to
get your home exactly right. While not all the details included below are
important for pricing, it makes sense to gather as much of the details as possible at
this time as it saves work later. It will also make for a smoother, faster and more
worry free construction phase.
3. It helps eliminate the potential for surprises due to a difference in assumptions
between the builder and the customer. If specifications are very detailed, it is rare
that we will come across an issue during construction where we disagree as to the
intent (and therefore the price). In short, it holds both the builder (and the
customer) accountable for what’s in this document.
4. Lastly, if you are getting other bids for this job, this detail will help you evaluate
the bids. For obvious reasons, it’s important for comparison purposes that each
bid contain the same scope of work. Since Berg Mountain Homes has spent a lot
of time developing this document, we do ask that you not share it with the other
bidders.
BERG MOUNTAIN HOMES
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Of course, we understand that not everything can be decided at this time. Often, the
decision for a certain feature will be based on price which is an unknown initially. So we
offer the opportunity for you to have options available. We’ll be glad to price something
several ways and allow you to make the decision at a later date. With respect to this
document, we will initially specify a feature a certain way and provide an overall price
making that assumption, but at the end of each section we’ll add other options for that
feature along with how that option will change the overall price. These options are
usually customer initiated, but occasionally we will add an option on our own initiative if
we think it might make sense and be of interest to the customer. If during the draft phase
of this proposal, you do make a decision on an option just let us know and we’ll modify
the specifications and pricing accordingly.
Additionally, allowances will be used in other areas where a final decision cannot be
reached. Of course, you will have typical allowances such as plumbing fixtures, lighting
fixtures, flooring, etc. But in some cases, we may provide allowances for other
construction items such as decking or masonry if we can’t be sure of the scope of that
item. Sometimes allowances will be in whole dollars and when it makes sense, they may
be based on measurements such as square or linear footage. Berg Mountain Homes tries
to make sure that allowances are healthy as we don’t want you to experience surprises in
the form of overages with respect to these allowances. Whenever possible, you should
attempt to validate the amounts of the allowances provided by doing a little bit of
shopping to see if what we provided seems to be reasonable for your tastes and wishes.
OK, enough talk, let’s get started…
[bookmark: _Toc80726009][bookmark: _Toc108882363]General
1. When this document is finalized (and you hopefully choose Berg Mountain
Homes as your builder), this document will be incorporated by reference
into the final Construction Agreement.
2. Unless amended in writing, please note that any specification made in this
proposal will supersede any blueprints, drawings, plans or verbal
discussions.
3. Construction materials and methods may vary from the blueprints or from
the construction notes provided in the blueprints; but at all times state
Residential Building Codes will be met or exceeded
4. Throughout this document, elevations (views from the side rather than
overhead) are given with the view side of the home being the rear elevation,
the opposite side being the front elevation (the street side) and then the left
and right elevations being from a front elevation perspective. All
dimensions are in format width x depth with a front elevation perspective.
5. To facilitate the eventual creation of work orders for the sub-contractors,
this document is organized generally by trade contractor and loosely follows
the home building construction schedule (that’s why it starts with sitework,
excavation and concrete).
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[bookmark: _Toc80726010][bookmark: _Toc108882364]Site work and Excavation
1. excavation of home site with backfill as needed to return site as near as
possible to original condition
2. 15’ setback from property lines to be maintained
3. if necessary, after house site excavation, local surveyor to mark house
corners to ensure no encroachment on setbacks (cost to be paid directly by
Customer)
4. Customer will identify locations for additional under brushing and tree
removal and will pay for cost outside the scope of this project
5. under brushing (removal to ground level of most brush and trees under 6” in
diameter) in area designated and agreed to between Builder and Customer
6. installing conventional (10” large diameter pipe) 3-bedroom septic system
(in accordance with Cherokee County permit dated ______); installation
includes removal of brush and trees as needed to install tank and drain lines
7. hydro seeding of steep banks exposed during basement excavation or
creation of driveway / parking area
8. gravel driveway and turnaround area; includes fill dirt sufficient to build up
driveway bank and/or turnaround area
9. private well at a suitable area near the main road – actual costs of the well to
be passed through to Customer
10. extending water from well/community water system to home
11. connection of electrical line from transformer to externally mounted meter
12. landscaping allowance = $2,500
Options:
• additional hydro seeding - $350 per tank (covers approximately 7,000
square feet) plus additional site work preparation costs (smoothing,
removal of stumps and stones, etc.)
Notes/Questions:
1.
[bookmark: _Toc80726011][bookmark: _Toc108882365]Concrete, Foundation and Slab
1. poured concrete stem wall (with footer) on view side as needed depending
on depth/location of virgin soil; allowance for stem wall = $_____ which
includes a ___’ tall ___56’ section of concrete (the full view side plus ___’
back on each side); an increase or decrease in the amount of the concrete
used in the stem wall will result in a $15/square foot cost adjustment
2. concrete footers around house perimeter – sized to code
3. footers as needed under interior load bearing walls
4. house footers that do not sit underneath concrete walls to be poured
monolithically with slab
5. poured concrete basement walls (8” thick) as needed to retain earth around
basement
6. concrete wall in basement bedroom to include formed opening for window
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7. retaining wall off _______ corner; allowance for retaining wall = $_____
which includes a ___’ tall ___’ section of wall; an increase or decrease in
the amount of concrete used in the stem wall will result in a $10/square foot
cost adjustment
8. retaining wall off _____ corner approximately sloping from 8' tall to 2' tall
and extending approximately 12' from house corner
9. estimated concrete wall sizes as follows:
a. stem wall – 6’ high x 70’ long
b. basement walls – 9’ high x 77’ long
c. left side retaining wall left side of house – 8’ high x 12’ long
10. if length of concrete walls exceeds estimated lengths, Customer will pay
additional costs as follows (Customer will also receive a credit if lengths are
less than estimated):
a. 3’ wall - $65 per linear foot
b. 4’ wall - $70
c. 5’ wall - $80
d. 6’ wall - $85
e. 7’ wall - $90
f. 8’ wall - $95
g. 9’ wall - $105
h. 10’ wall - $115
11. if height of concrete walls exceeds estimated heights, Customer will pay
additional costs calculated using the difference between the estimated height
and the actual height in accordance with the above price schedule (Customer
will also receive a credit if heights are less than estimated)
12. chases in basement concrete walls as needed for water lines, gas lines,
electrical and drain lines
13. concrete slab as basement / garage floor with 6” x 6” #10 welded wire mesh
14. concrete stoop off kitchen entry (approx. 4’ x 6’)
15. termite treatment beneath slab
16. waterproofing of all below grade concrete walls (including footer level
drainage system) – 5 yr. warranty
Notes/Questions:
1.
[bookmark: _Toc80726012][bookmark: _Toc108882366]Framing
1. square footage:
a. main floor to have _____ finished sqft
b. 2nd floor to have ____ finished sqft
c. basement to have ____ finished sqft
d. basement to have ____ partially finished sqft
e. basement to have ____ unfinished sqft
f. ____ sqft attached/detached garage
g. total finished area ____ sqft
h. total partially finished area ____ sqft
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i. total unfinished area ____ sqft
2. roof structure:
a. 12 / 8 pitch roof with single ridge beam and gable ends
b. (2) front dormers with 12/12 pitch
c. front covered porch with 9/12 pitch
d. shed roof with 4/12 pitch over rear deck
e. 16" soffits
f. stick framed roof or roof trusses
g. OSB roof sheathing with Titanium brand underlayment (eliminates
need for felt)
h. roof sheathing with a reflective radiant barrier with Titanium brand
underlayment
3. ceilings:
a. vaulted ceiling in great room, and foyer; all other main floor
ceiling heights at 8’
b. vaulted ceiling in loft; all other 2nd floor ceiling height at 8’
c. basement ceiling height to be minimum 8'
4. walls:
a. exterior walls to be 2x6 16” on-center with 7/16” (or thicker)
sheathing
b. interior walls to be 2x4 24” on-center (with 2x6 or closer spacing if
needed for load bearing capacity)
c. insulation walls against basement concrete to be 2x2’s
d. full house wrap and taping of all house wrap joints and around
windows and doors
e. 7/16" Huber zip system for exterior wall; fully taped and sealed
(eliminates need for house wrap) – for details on this system, see:

5. floor system:
a. floor system between basement and main floor to be open web
trusses
b. floor system between basement and main floor to be conventional
framing or I-joists with HVAC chases…
c. floor system between first floor and second floor to be open web
trusses
d. floor system between first floor and second floor to be
conventional framing or I-joists with HVAC chases…
e. 3/4" floor sheathing glued and screwed to floor system
Options:
1. roof sheathing with a reflective radiant barrier underneath (see LP
Tech Shield for an example) to reduce radiant heat from the sun and
reduce energy costs 10-15% - very good for vaulted ceiling
applications) – add $____; see 
Notes/Questions:
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1.
[bookmark: _Toc80726013][bookmark: _Toc108882367]Exterior
1. siding and trim:
a. fiber cement board lap siding on all exterior walls with the
exception of:
• fiber cement board shake shingle accents in all gable
ends (including dormers)
b. Migrate (or similar water resistant textured material) trim (3" x
5/4" thick, fascia (4/4" thick) and standouts for hose bibs, exterior
lighting, etc.
c. textured fiber cement board soffit and venting to code
d. siding / trim to be painted on-site with three colors (base color,
shingle accent color and trim color) and optional alternative color
for exterior doors
2. exterior masonry:
a. stacked rock around great room entry door
b. stacked rock ‘columns’ at view side basement corners
c. stacked rock 42” up the wall on lower portion of view side
basement wall with angled water table cap rock
d. all stacked rock to be cultured stone
e. fieldstone (flat rock) on any other exposed above grade concrete
f. painted textured stucco on any other visible above grade concrete
3. 30-year warranty (minimum) architectural shingle roofing
4. gutters / downspouts to compliment house / roof color; no gutter covers
5. downspouts to feed into drainage system to direct water away from house
6. garage doors and exterior doors painted to compliment house / roof color
7. rear deck (____ sqft) as follows:
a. pressure-treated undercarriage
b. 5/4 x 6" wide pressure treated decking screwed to undercarriage
c. pressure treated rail system with ¾” powder coated aluminum
balusters (painted black)
d. pressure treated rail system including 2x2 pickets
e. copper post caps (12 units)
8. front covered porch (____ sqft) as follows:
a. pressure-treated undercarriage
b. 5/4 x 6" wide pressure treated decking screwed to undercarriage
c. pressure treated rail system with ¾” powder coated aluminum
balusters (painted black)
d. stained tongue and groove ceiling – 4” bead spacing
e. painted bead board ceiling
9. deck stairs to include 2x12” beauty band and riser front
10. pre-braced open deck area off corner of master bedroom to accommodate
future hot tub
Options:
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• metal roof – add $_______
• ice dam protection (a 6' wide waterproof barrier on the north side eaves
of the house) – add $300; for product details, see

• rockwork not listed above – add
• artificial rock (any) - $14 per square foot
• veneer rock (flat rock applied to vertical surfaces) - $11 per
square foot
• screened-in rear porch – add $______
• composite decking (Terex or similar) – add $______
• glass panels instead of conventional hand rail system – add $300 per 8’
section
• decks and stairs not listed above - add
• $13 per square foot of deck surface
• $48 per step
• $20 per linear foot of deck and stair rail
Notes/Questions:
1.
[bookmark: _Toc80726014][bookmark: _Toc108882368]Interior
1. insulation in finished areas as follows:
• R21 blown-in cellulose insulation in exterior framed walls and
any interior framed walls that adjoin unfinished areas
• R5 blown-in cellulose insulation in 2x2 framed cavity in all
exterior concrete walls
• R38 blown-in cellulose insulation in roof
• no insulation in interior walls
2. insulation in unfinished areas as follows:
• batt insulation as required by code in ceilings and in framed
walls separating unfinished space from finished space
3. all window and door openings sealed with foam sealant
4. all walls and ceiling to be dry walled except for:
• tongue and groove ceilings
• bead board ceilings
• mechanical room ceiling (open)
• unfinished basement areas
5. all drywall glued and screwed to studs
6. all drywall finished with light knockdown texture except as follows:
• tape and flat finish of garage walls
• fire tape of partially finished basement area
7. paint as follows:
• no paint on fire taped drywall areas
• one coat of drywall primer on garage walls and ceiling
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• all other areas painted with one coat of drywall primer on walls
and one coat of white paint on ceiling; one coat of flat latex
color on all walls; two wall paint colors
8. upgraded trim (1” x 4” base with bevel; 1 x 4” door and window trim with
dog-eared top piece, and window sills) except as follows:
• garage to receive white painted utility trim
• no trim in partially finished or unfinished basement
9. ¾” tongue and groove wood ceiling with 4” bead spacing in great room,
master bedroom and master bathroom
10. painted bead board ceilings (with OSB underlayment for rigidity) in kitchen,
dining room and master bedroom
11. stairs and loft railings to be combination pine posts and rails and wrought
iron balusters (combination of single basket, double basket and twist)
12. stairs and loft railings to be standard pine posts, rails and pickets
13. stairs and loft railings to have enhanced trim package
14. all woodwork (including baseboard, window and door trim, interior side of
any wood windows, interior mountains, railing systems, exposed beams, collar
ties and tongue and groove ceiling and paneling) to be stained and finished
with lacquer
Options:
• paint wall vents and stair lights to match wall color – add $100 per color
Notes/Questions:
1.
[bookmark: _Toc80726015][bookmark: _Toc108882369]Flooring
1. unfinished garage floor
2. attic crawl space to have several sheets of plywood
3. epoxy paint on garage floor
4. epoxy paint on mechanical room floor
5. tile floor in all bathrooms and laundry room; material allowance (including
tile, accent pieces, bullnose and grout) = $_____ (approx. $___ per square
foot)
6. wood floor throughout the rest of the main floor; material allowance =
$_______ (approximately $____ per square foot)
7. note on wood floor installation – if the width of the individual planks chosen
for the floor is less than 3”, add $0.50 per square foot
8. carpet in all other areas of basement and 2nd floor and on both sets of stairs;
material allowance (including pad) = $_______ (approximately $____ per
square yard)
Note: all allowances include tax and delivery
Options:
• for tile patterns and diagonal installation – add $1 per square foot
Berg Mountain Homes – copyright 2005 to present Proposal
______ proposal page 9 of 21 customer initials _____ _____
builder initials _____
• for natural stone (travertine, tumbled marble, slate) tile – add $2 per
square foot (natural stone requires more sorting time, cutting time
[each piece must be cut with a tile saw] and all natural stone must be
sealed)
Notes/Questions:
1.
[bookmark: _Toc80726016][bookmark: _Toc108882370]Doors
1. standard hardware (knobs or handles) with matching hinges and doorstops
2. interior doors to have privacy locks on all bedrooms and bathrooms and
passage locks elsewhere
3. exterior doors to have standard one side keyed deadbolt
4. front entrance door to have upgraded handle set
5. solid 6-panel pine interior doors with stain and finish to match trim
• (8) standard doors
• (5) bi-folds
• (1) French
• (4) pocket
6. exterior door summary:
• (2) 6-panel solid steel
• (1) ¾-lite decorate oval textured fiberglass with matching sidelights
• (1) half-lite rectangular 9-lite textured fiberglass
• (2) full-lite rectangular blinds between the glass smooth fiberglass
• (2) full-lite rectangular textured fiberglass French doors
• (1) standard 2 car 16’ x 7’ insulated garage door with row of glass
panels
Options:
• door screens – Customer may provide and Builder will install at $100
per door
• additional doors = cost of door plus $250 (framing, hanging, trim
material, trim labor, paint/stain of trim, paint/stain of door and door
hardware)
Notes/Questions:
1.
[bookmark: _Toc80726017][bookmark: _Toc108882371]Windows
1. operable windows to be Atrium brand premium vinyl (Energy Star
designated with Low-E coating and argon gas insulation); no grids or
shutters; all to have lift out screens
• (1) awning
• (6) single hung (lower level)
• (2) twin single hung (lower level)
• (5) double hung (upper level)
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• (2) casements
• (2) double casements
• (1) slider
2. fixed windows (14 units) to be made locally to fit specifications with
exception of bay window fixed panels which need to match flanking
operable windows; windows to have Low-E coating and bronze tinting
3. (2) sky lights in master closet
4. (1) solar tube in upstairs guest bathroom
5. (1) window well for basement bedroom egress window
Options:
• tinting of fixed windows – add $____
• additional windows = cost of window plus $150 (framing, installing,
trim material, trim labor and paint/stain of trim)
Notes/Questions:
1.
[bookmark: _Toc80726018][bookmark: _Toc108882372]Kitchen
1. knotty pine cabinets with the following features (final layout to be
determined):
• full refrigerator depth cabinet above refrigerator
• framed wall with drywall separating refrigerator from hallway
• raised corner cabinet with glass front
• pull out trash can with mechanism attached to cabinet door
• lazy Susan in lower corner cabinet
• full-extension drawer glides on all drawers
• range hood with venting to exterior
• valance over sink
2. kitchen cabinetry allowance = $______ (including knobs, pulls, range hood
and installation)
3. granite countertops with 4” granite backsplash except for behind range and
sink where this should go all the way up to either the cabinet or window
above; material allowance = $_______ (approx. $____ per foot)
4. appliances (including range, oven, microwave, dishwasher, garbage
disposal, refrigerator, washer, dryer) to be selected and paid for by
Customer separate from this project; Customer will also pay for delivery
costs; typically, installation is part of the service provided by the appliance
supplier – if Builder has to install; Builder will add $25 per appliance to
cover the cost of installation
Notes/Questions:
1. I left in a few of the kitchen options that I thought would look nice or
add functionality. if you don’t want these please let me know. this is
really just a starting point for pricing purposes. you’ll have full
control over the layout and options when the time comes
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Bathrooms and Laundry Room
Powder Room
1. 30” vanity with standard grade (oak, maple) stained cabinets; vanity to be
comfort height (36”); allowance = $_____ (allowance includes cultured
marble countertop)
2. granite counter with 4” backsplash; material allowance = $_______ (approx.
$____ per foot); includes sink provided by countertop company
3. cultured marble countertop with integrated sink and 4” backsplash; countertop
included in cabinetry allowance above
4. single undercount sink
5. pedestal sink
6. elongated 1.6 gym or lower toilet
7. Customer to provide mirror and bathroom accessories and Builder to install
[bookmark: _Toc80726019][bookmark: _Toc108882373]Master Bath
1. 60” vanity with standard grade (oak, maple) stained cabinets; vanity to be
comfort height (36”); allowance = $_____ (allowance includes cultured
marble countertop)
2. granite countertop with 4” granite backsplash; material allowance = $_______
(approx. $____ per foot); includes sink provided by countertop company
3. cultured marble countertop with integrated dual sink and 4” backsplash;
countertop included in cabinetry allowance above
4. dual under mount sinks
5. 60” x 36” rectangular jetted tub with tile surround (motor access _____)
6. oversized tile shower with glass door framed to match plumbing fixtures,
bench and built-in soap and shampoo platforms; tile to extend to ___
7. tub and shower tile material allowance (including tile, accent pieces, bullnose,
grout, and surface mounted soap and shampoo platforms) = $_____ (approx.
___ sq feet x $4 per sq foot)
8. elongated 1.6 gym or lower toilet
9. Customer to provide mirror and bathroom accessories and Builder to install
[bookmark: _Toc80726020][bookmark: _Toc108882374]Guest Baths
1. 42” vanity with standard grade (oak, maple) stained cabinets; vanity to be
comfort height (36”); allowance = $_____ (allowance includes cultured
marble countertop)
2. granite countertop with 4” granite backsplash; material allowance = $_______
(approx. $____ per foot); includes sink provided by countertop company
3. cultured marble countertops with integrated sink and 4" backsplash;
countertop included in cabinetry allowance above
4. single undercount sink
5. 60” x 36” one-piece fiberglass tub/shower combination with simulated tile
surround
6. 60” x 36” drop-in tub with tile shower surround to 7’ high
7. no door on tub/shower
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8. tiled shower in with tile ¾ of the way to the ceiling and glass door with frame
to match plumbing fixtures; no tub
9. tub and shower tile material allowance (including tile, accent pieces, bullnose,
grout, and surface mounted soap and shampoo platforms) = $_____ (approx.
___ sq feet x $4 per sq foot)
10. elongated 1.6 gpm or lower toilet
11. full width mirror
12. Customer to provide bathroom accessories and Builder to install
Basement Bath
1. stubbed for pedestal sink, shower and toilet
Laundry Room
1. 36” laundry tub cabinet base with Formica top; countertop allowance = $___
2. 60” cabinets over washer/dryer
3. laundry room cabinetry allowance = $____
Options:
• for tile patterns and diagonal installation – add $1 per square foot
• for natural stone (travertine, tumbled marble, slate) tile – add $2 per
square foot (natural stone requires more sorting time, cutting time
[each piece must be cut with a tile saw] and all natural stone must be
sealed)
• for built-in niches in tiled showers - add $100
• for benches in tiled showers – add $200
• upgrade powder room countertop to granite – add $____
• upgrade master bath countertop to granite – add $____
Notes/Questions:
1.
[bookmark: _Toc80726021][bookmark: _Toc108882375]Built-Ins and Shelving
Built-Ins
1. stereo cabinet in great room – location/design to be determined
2. bay window seat (to be hinged and open to storage below)
3. lower pullout drawer base for washer / dryer
4. bookcases (36” x 7’ tall) with doors on base cabinet and shelving above
flanking fireplace
5. built-in cabinetry allowance = $_____
6. built-in countertop allowance = $_____
[bookmark: _Toc80726022][bookmark: _Toc108882376]Shelving
1. closet shelving to be pine and stained / finished to match trim; no wire
shelving
2. open shelving in 2nd floor linen closet
3. linen shelving in master closet
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4. rod and shelf in 2nd floor bedroom closet
5. rod and shelf in mud room coat closet
6. pantry shelving (5 unit’s x 18” deep)
Notes/Questions:
1.
[bookmark: _Toc80726023][bookmark: _Toc108882377]Plumbing
1. thankless hot water heater
2. electric hot water heater with cutoff switch in laundry room
3. pre-plumb for water softener in case needed in the future
4. floor drain in mechanical room
5. two outside frost proof hose bibs
6. exterior hose bibs to be on separate shutoff
7. pre-plumb for future wet bar in rec room (directly behind bathroom)
8. pre-plumb for future bathroom in basement (toilet, vanity, shower)
9. pre-plumb for sink in future outside kitchen area
10. kitchen sink water purifier hookup
11. additional plumbing = $150 per drop
• a hose bib = 1 leg
• an additional showerhead in an existing shower = 1 drop
• a fixture with a drain = 2 drops
Tub and Shower Allowance - $_____ (approx. item costs below)
• (1) jetted tub - $850
• (1) drop-in tub / shower combination - $600
• (2) tubs - $800
Plumbing Fixture Allowance - $_____ (approx. item costs below)
• (4) toilets (elongated) - $800
• (2) bathroom sinks - $200 (cultured marble tops have integrated sinks)
• (1) powder room pedestal sink - $200
• (5) bathroom faucets - $750
• (2) shower faucets - $400
• (1) full-body shower system - $1,250
• (1) roman/tub faucet - $350
• (1) kitchen sink (cast iron or acrylic undercount) - $500
• (1) kitchen sink (stainless) - $300
• (1) kitchen sink (farmhouse/apron front) - $1,000
• (1) kitchen faucet - $300
• (1) prep sink (stainless undercount) - $150
• (1) prep sink faucet - $150
• (1) laundry tub - $100
• (1) laundry tub faucet - $100
• (1) garbage disposal - $150 (note: septic systems are sensitive to the
types of waste entering the system and while using a disposal is
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acceptable, it is important to be educated on its effect on your septic
system as well as on the proper care and maintenance of the system)
Notes/Questions:
1.
[bookmark: _Toc80726024][bookmark: _Toc108882378]Electrical
1. minimum 200-amp electrical service
2. four external electrical outlets
3. transfer switch for portable generator; Customer to provide list of circuits
that will run from generator
4. speaker wiring at 4 external locations on deck and run to central location in
home
5. pre-wire for 5.1 or 7.1 media in great room with rear speakers, sub-woofer
and TV mounted over fireplace; run wires to central location to be
determined
6. neither the cost of nor the installation of any audio / video equipment
(including but not limited to speakers, components, volume controls, remote
sensing or termination units, mounting brackets, racks, etc) is included
7. (1) floor outlet in concrete slab in basement
8. (1) floor outlet in great room floor
9. one phone jack
10. one television drop in each bedroom and in great room
11. switched outlets in all bedrooms
12. wall outlets to code
13. additional wiring = $50 per leg
• an outlet = 1 leg
• a light with a switch = 2 legs
• a light added on an existing switch = 1 leg
• a phone jack = 1 leg
• an additional TV location = 2 legs (since we bring to wires to each
location)
• speaker drop = 1 leg per speaker
• speaker drop with intermediate volume control = 2 legs
14. standard toggle switches with the exception of dimmer switches in key areas
15. standard switch and outlet cover plates
16. pre-wiring of hot tub sub-panel (does not include labor or material to
connect to hot tub and does not include breaker in electrical panel as breaker
size varies by hot tub manufacturer/model)
17. pre-wiring for fireplace blowers
18. pre-wiring for whirlpool tub heater
19. pre-wiring for wet bar fridge
20. pre-wiring for flat screen TV above great room fireplace – including
extension of wiring to remote location of audio/video components
21. pre-wiring for television outlets, phone outlets and satellite dish
22. pre-wiring for satellite internet to central wireless router location
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23. termination of phone lines and telephone punch block in mechanical room
24. all tv and phone drops run to central location in the mechanical room
Lighting and Fans Allowance - $_____ total (approx. item costs below):
• (1) dining room light - $250
• (1) foyer hanging light - $150
• (1) kitchen island hanging 3 light fixture - $150
• (3) kitchen pendant lights over barstool area = $300
• (5) bathroom vanity lights - $500
• (2) bathroom ceiling lights (master bath and guest bath) - $100
• (5) interior fans with light kits and light/fan on separate switch (1
master bedroom, 2 guest bedrooms, 1 great room) - $750
• (2) exterior fans under covered porch - $400
• (2) sconces (stairs between 1st and 2nd floor) - $150
• (2) spot lights (over great room fireplace) - $100
• (5) exterior wall mounted lights (2 either side of garage door, 2 either
side of great room entry door, 1 with motion sensor next to kitchen
entry door) - $250
• (1) doorbell/chime - $100
Builder Provided Lighting - These items will not be part of the allowance:
• (2) flood lights with motion sensor
• (4) flood lights without motion sensors
• (4) utility/closet lights (master closet, guest closet, guest closet, pantry)
– finish to match door knobs/hinges
• (2) under cabinet lights in kitchen
• (1) over sink light in kitchen
• above cabinet accent lighting in kitchen
• (8) recessed can lights in basement (2 exercise room, 4 offices, 2
laundry, 2 on stairs to main) – white trim kit
• (10) recessed can lights on 1st floor (4 hallways, 6 kitchen)
• (3) recessed can lights on 2nd floor (hallway)
• (2) recessed spot lights (over basement fireplace)
• (4) shower recessed can lights (2 master shower, 2 guest shower)
• (1) bare bulb (mechanical room)
• (2) vents (powder room, master bathroom)
• (2) combo heat / vent / light units (guest bathrooms)
• (2) long fluorescents (garage)
• (4) short fluorescents (mud room closet, 2 upstairs bedroom closet,
under stairs closet in basement)
• (1) garage door opener
• receptacle in center of rec room area for future pool table light
• smoke detectors as required by code
• carbon monoxide detectors (1 per floor)
• all can trim kits to be white with exception of trim kits on wood
ceilings; these will be ___________ to match the ___________
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• all cans to be insulation contact
• all incandescent and fluorescent bulbs
Options:
• electric radiant floor heat in master bathroom (not including closet) –
add $______
• pre-wire for alarm system (up to 12 devices) - $500
Notes/Questions:
1.
[bookmark: _Toc80726025][bookmark: _Toc108882379]HVAC and Utilities
1. full contained mechanical room with gas hookups, water shutoff,
telecommunication hookups, satellite distribution, electrical panel, HVAC and
water heater
2. electric heat pump – single unit with variable speed air handler and 3 zones
(one for each floor); minimum 13 SEER
3. energy recovery ventilator for bringing fresh air into house
4. HVAC allowance (including ventilator) = $_____
5. venting to exterior:
a. dryer vent (including recessed dryer vent box)
b. range vent to exterior
c. bathroom vents
Options:
• geothermal HVAC system – add approximately $______ additional cost
• whole house humidifier attached to HVAC system – add $______
• enhanced HVAC air filter (replaceable 5” media filter) – add $______
• air purifier (electrostatic with serviceable filter) – add $_______
• upgraded floor registers (brushed nickel / oil rubbed bronze) – add $300
Notes/Questions:
1.
[bookmark: _Toc80726026][bookmark: _Toc108882380]Fireplaces
1. master bedroom fireplace – gas burning corner fireplace; vented directly
through outside wall; sheetrock front, wood trim and oversized wood top
2. great room fireplace – gas burning fireplace; vented through roof with no
chimney; full height artificial stacked rock masonry with hearth and mantle;
top of firebox opening to be arched with keystone and voussoirs on either side
of the keystone; hidden wiring and installation of Customer provided support
brackets for future flat screen TV
3. fireplace allowance (allowance covers all costs except installation – including
firebox, inserts, face/face kit, log set, andirons, starter, blower, auxiliary
blower, remote, thermostat, conversion to propane, all piping, termination
caps and wood mantles) = $_____
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4. fireplace masonry allowance (allowance includes cost of all materials and
installation of fireplace rockwork, hearth and mantle) = $____; including cost
of wood mantle, arched firebox opening and recessed area for TV
Notes/Questions:
1.
[bookmark: _Toc80726027][bookmark: _Toc108882381]Gas Piping
1. installation of propane manifold in mechanical room with a stub out to
exterior of home (for future connection to tank) and distribution to the
following areas (with shutoffs at each location):
• laundry room for dryer
• thankless hot water heater
• kitchen stove
• two fireplaces
• grill on deck
2. additional gas locations are $300 per drop
3. Customer to contract with local propane supplier to purchase or lease propane
tank and arrange for gas delivery contract; Builder to bury propane if
delivered prior to final grading; Customer to arrange for hookup of propane
tank to house and startup of fireplaces subsequent to occupancy
Notes/Questions:
1.
[bookmark: _Toc80726028][bookmark: _Toc108882382]Job Costs (included in estimate)
1. applicable building permits (excluding well and septic permits, if
applicable)
2. temporary electrical hookup from transformer if transformer is within 250
feet of house; Customer is responsible for costs of bringing transformer to
within 250 feet of house (this is not included because it customarily
provided by the developer)
3. temporary electricity usage while house is under construction as well as
permanent electrical hookup
Note: at start of project, Customer agrees to set up an account with
the local power company in Customer’s name and will receive and
pay bills each month (including cost for permanent power
hookup); at end of project and upon receipt of bill copies, Builder
will deduct these costs from amounts owed by Customer
4. job toilet during duration of project
5. cleanup of job site and inside of home prior to occupancy
6. builder’s risk insurance (covering the value of the unfinished house - $5,000
deductible)
7. general liability insurance and worker’s compensation insurance for Builder,
Builder’s employees and Builder’ sub-contractors
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[bookmark: _Toc80726029][bookmark: _Toc108882383]Proposal Excludes
These are the responsibility of the Customer and are not included in the proposal.
1. design costs related to final revisions of house plans / elevations
2. financing costs associated with construction or permanent loans
3. liability insurance protecting Customer (Builder has general liability
policy that covers Builder and sub-contractors – see the Insurance
section below for more information on this subject)
4. worker's compensation insurance on behalf of uninsured subcontractors
paid directly by Customer
5. builder's risk insurance – Customer to buy directly
6. homeowner’s association design review fees or design compliance
deposits
7. survey costs, if needed, to accurately locate property lines
8. engineering costs if required by local building department
9. cost of the on-site well and pump
10. additional costs of septic system if, when permit is obtained, the system
is not a standard conventional system?
11. fees associated with connection to community water system
12. appliances (including range, oven, microwave, dishwasher, refrigerator,
garbage disposal, washer, dryer) – Customer will purchase separately
(and pay for cost of delivery) and Builder will facilitate delivery and if
installation is performed by Builder, Builder will charge $25 per
appliance
13. propane tank and hookup of propane tank to house
14. telephone hookup
15. satellite dish (television and/or DSL) and hookup
16. neither the cost of nor the installation of any audio / video equipment
(including but not limited to speakers, components, volume controls,
remote sensing or termination units, mounting brackets, racks, etc.)
17. mailbox
18. bathroom accessories (towel bars, toilet paper holders) – Customer will
purchase separately and provide for Builder to install
19. master bath mirrors (2) and powder room mirror – Customer will
purchase separately and provide for Builder to install
20. brackets for mounting possible over fireplace TV
21. deck stain (not recommended until pressure treated lumber has dried –
approximately 9 to 12 months)
22. labor or material to connect hot tub pre-wiring to actual hot tub
23. breaker in electrical panel for hot tub as breaker size varies by hot tub
manufacturer/model
24. additional under brushing and tree removal as requested by Customer
25. additional construction costs as a direct result of building code changes
made subsequent to the signing of this document
26. any additional expenses incurred due to any unexpected or unforeseen
site conditions including but not limited to:
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a. additional excavation expenses incurred due to any condition
below the surface of the ground presenting unusual problems
(such as undiggable rock / shale or the presence of springs /
other water sources)
b. additional costs if radon gas is discovered on site
c. additional cost for water filtration, if needed or desired
27. any additional expenses incurred due to force majeure (extraordinary
events or circumstances beyond the control of Builder such as war,
crime or “Acts of God” including but not limited to earthquake, floods,
lighting, landslides, etc.)
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[bookmark: _Toc80726030][bookmark: _Toc108882384]Allowance Recap
1. per schedule concrete retaining walls
2. $_____ landscaping
3. $_____ interior doors
4. $_____ exterior doors
5. $_____ windows
6. $_____ door hardware
7. $_____ appliances
8. $_____ cabinetry, including:
a. $_____ kitchen
b. $_____ master bath
c. $_____ guest baths
d. $_____ powder room
e. $_____ laundry room
f. $_____ built-ins
9. $_____ countertops, including:
a. $_____ kitchen
b. $_____ master bath
c. $_____ guest baths
d. $_____ powder room
e. $_____ laundry room
f. $_____ built-ins
10. $_____ bathroom accessories
11. $_____ bathroom mirrors
12. $_____ tile and grout, including:
a. $_____ flooring
b. $_____ kitchen backsplash
c. $_____ master bath tub and shower
d. $_____ guest baths tub and shower
13. $_____ wood flooring
14. $_____ carpet
15. $_____ plumbing fixtures (excluding tubs/showers)
16. $_____ tubs/showers
17. $_____ lights and fans (exclusive of Builder provided items)
18. $_____ fireplaces
19. $_____ fireplace masonry
Note: all allowances include tax and delivery
[bookmark: _Toc80726031][bookmark: _Toc108882385]Warranty, Insurance and Change Order Policies
Please note the following Berg Mountain Home policies:
Warranty – all Berg Mountain Homes come with an 18-month warranty.
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Insurance – Berg Mountain Homes carries both general liability and workers
compensation insurance. If one of our sub-contractors is uninsured for either general
liability or worker’s compensation, Berg Mountain Homes will provide that insurance
on behalf of the uninsured subcontractor. However, this insurance does not replace
the Customer’s need for their own coverage. We recommend that you check with
your insurance agent to make sure you are aware of your options.
Changes – Any Change Order that results in additional project costs and whose cost is
not otherwise specified in this proposal will be billed to Customer at actual cost plus
15%. Excluded from this 15% charge are any overages on material allowance items
such as lighting fixtures, plumbing fixtures, etc.
Change Order Administrative Fees – The first twenty (20) changes are included in the
price of the home below. After the first twenty (20) changes, each additional Change
Order will result in a $50 administrative fee.
Copies of Berg Mountain Homes documents (including the Construction Agreement
and Warranty) can be found on the Berg Mountain Home web site.
[bookmark: _Toc80726032][bookmark: _Toc108882386]Proposal
Berg Mountain Homes proposes to build the home described above for an all
inclusive price of $________. This price includes all Berg Mountain Home fees -
including design, project management, accounting, reporting, construction
scheduling, supervision, and quality assurance.
The only changes to the price you will pay for your home could be as follows:
1. Changes made to the project scope subsequent to the signing of this
document.
2. Differences between the Allowances outlined above and the actual price of
those items.
The next step in the building process is to agree to this proposal (including any
changes we’ve noted during our discussion of this document) and subsequently to
sign the Construction Agreement (which references this document as an attachment).
Customer (sign and date) ______________________________________
Customer (sign and date) ______________________________________
Builder (sign and date) ______________________________________
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